Configuring the PFC POP Trigger

Basic Parameters tab:

- DAC IC: the period synchronization value as a unitless signed 32-bit integer. In conjunction with the current range parameter, determines the initial condition of ISYNC. During a POP analysis, ISYNC is always held at this value. At the end of a transient analysis, the 32-bit signed integer value - DAC_sync - corresponding to the determined ISYNC required to synchronize the circuit will be written to this parameter, overwriting any previous value entered by the user.
- Vout: The PFC rectifier circuit output voltage.
- Input type: Select AC if the PFC is being simulated with AC input. Select DC otherwise, in which case the PFC POP Trigger behaves just like a regular POP Trigger.