Conclusion

- From version 9.1d, the PFC POP Trigger Schematic device can be used to successfully perform POP and AC analysis on AC-DC PFC rectifer circuits for which POP analysis would previously fail.
- For many PFC schematics, users are no longer limited to AC analysis with DC input or DVM Multi-Tone Analysis. Just like for many DC-DC converters, now users can perform SIMPLIS' bench-emulating time-domain AC analysis on AC-DC circuits.
- Next Webinar (June 15th, 2023):
  - DVM Testplan Wizards and Editor
  - https://simplis.com/webinar/2023/06/15/dvm-testplan-wizards-and-editor