Advanced Parameters tab:

- Loop gain: Determines the speed of the synchronization.
- Current gain: A value specifying by how much the PFC target current changes for each incremental change in ISYNC. This value will vary greatly from circuit to circuit.
- Automatically calculate gain: Check this to disregard the value entered for the current gain above and calculate it automatically during the characterization step. If the box is checked, at the end of the transient automatically calculated gain will be written into the current gain parameter field above.
- Current range: Sets ISYNC range to be from -0.5*current range to +0.5*current range. The appropriate current range varies highly from circuit to circuit and it is recommended to check the box below (Automatically calculate range) to calculate it automatically.