baseschematic: ..\..\..\..\..\..\4_multi_tone.sxsch
log_file: ..\..\..\..\dvm_advanced.log
simulator: simplis
screenshot: schematic.png
deck: input.deck
init: input.deck.init
test_argument: Bode Plot|DC Input|Multi-Tone|NLB multiplier
datetimestamp: 11/17/2016 11:29 AM
status: RUN
spec: Min_VLOAD=pass,Min. Output1 Voltage (398.459) is greater than or equal to Min. Output1 Voltage Spec (380)
spec: Max_VLOAD=pass,Max. Output1 Voltage (401.144) is less than or equal to Max. Output1 Voltage Spec (420)
stats: N/A
numgraphs: 6
graphid: 63
graphname: new#tran
sg: simplis_tran3_63
path: simplis_tran3_63.sxgph
graphid: 68
graphname: default#68#tran
sg: simplis_tran3_68
path: simplis_tran3_68.sxgph
scalar: Max(VSRC)=114.294
scalar: Avg(VSRC)=114.263
scalar: Min(VSRC)=114.235
scalar: Pk2Pk(VSRC)=59.0359m
scalar: RMS(VSRC)=114.263
scalar: RMS(ISRC)=1.84198
scalar: Pk2Pk(ISRC)=147.59m
scalar: Min(ISRC)=1.7646
scalar: Avg(ISRC)=1.84153
scalar: Max(ISRC)=1.91219
graphid: 73
graphname: DVM SRC#tran
sg: simplis_tran3_73
path: simplis_tran3_73.sxgph
curve77:VSRC,FF0000
curve83:ISRC,008000
png: simplis_tran3_73.png
scalar: Max(VLOAD)=401.144
scalar: Avg(VLOAD)=400.093
scalar: Min(VLOAD)=398.459
scalar: Pk2Pk(VLOAD)=2.68493
scalar: RMS(VLOAD)=400.094
scalar: Max(ILOAD)=501.43m
scalar: Avg(ILOAD)=500.116m
scalar: Min(ILOAD)=498.074m
scalar: Pk2Pk(ILOAD)=3.35616m
scalar: RMS(ILOAD)=500.117m
graphid: 78
graphname: DVM LOAD#tran
sg: simplis_tran3_78
path: simplis_tran3_78.sxgph
curve82:VLOAD,FF0000
curve85:ILOAD,008000
png: simplis_tran3_78.png
graphid: 87
graphname: AC#tran
sg: simplis_tran3_87
path: simplis_tran3_87.sxgph
curve91:IL,FF0000
png: simplis_tran3_87.png
scalar: min_phase=10.9935
scalar: min_phase_freq=50
scalar: phase_crossover_freq=Unable to determine phase_crossover_freq
scalar: phase_margin=48.3828
scalar: gain_crossover_freq=11.2477
scalar: gain_margin=Unable to determine gain_margin
graphid: 93
graphname: DVM Bode Plot
sg: simplis_Multi_ToneAC1_93
path: simplis_Multi_ToneAC1_93.sxgph
curve97:PHASE,FF0000
curve99:GAIN,008000
png: simplis_Multi_ToneAC1_93.png
spec: min_gain_margin=warn,Unable to determine min_gain_margin
spec: min_phase_margin=pass,Phase Margin (48.3828) is greater than Min. Phase Margin (35)
rstatus: WARN
