back to overview ▲

### » DVM Test Report: Bode Plot|DC Input|POP-AC|PWM multiplier

Test Details |
Schematic | 4_multi_tone.sxsch
Test | Bode Plot|DC Input|POP-AC|PWM multiplier
Date / Time | 11/17/2016 11:30 AM
Report Directory | DVM_REPORTS\2016-11-17-11_20_AM\Bode Plot\DC Input\POP-AC\PWM multiplier
Log File | report.txt
Screenshot | schematic.png
Status | WARN
Simulator | simplis
Deck | input.deck
Init | input.deck.init
Measured Scalar Values |
Efficiency | 95.0946%
gain_crossover_freq | 11.3576
gain_margin | Unable to determine gain_margin
ILOAD | AVG 500.116m MIN 500.085m MAX 500.172m RMS 500.116m PK2PK 87.6286u
ISRC | AVG 1.84149 MIN 1.84144 MAX 1.84154 RMS 1.84149 PK2PK 101.347u
min_phase | 10.7993
min_phase_freq | 50
phase_crossover_freq | Unable to determine phase_crossover_freq
phase_margin | 49.131
Power(LOAD) | 200.093
Power(SRC) | 210.415
VLOAD | AVG 400.093 MIN 400.068 MAX 400.138 RMS 400.093 PK2PK 70.1029m
VSRC | AVG 114.263 MIN 114.263 MAX 114.263 RMS 114.263 PK2PK 40.5387u
Measured Spec Values |
Max_VLOAD | PASS: Max. Output1 Voltage (400.138) is less than or equal to Max. Output1 Voltage Spec (420)
Min_VLOAD | PASS: Min. Output1 Voltage (400.068) is greater than or equal to Min. Output1 Voltage Spec (380)
min_gain_margin | WARN: Unable to determine min_gain_margin
min_phase_margin | PASS: Phase Margin (49.131) is greater than Min. Phase Margin (35)
Bode Plot GAIN PHASE
SXGPH File | simplis_ac1_131.sxgph
AC IL
SXGPH File | simplis_pop1_125.sxgph
LOAD VLOAD ILOAD
SXGPH File | simplis_pop1_116.sxgph
SRC VSRC ISRC
SXGPH File | simplis_pop1_111.sxgph
Other SXGPH Files |
default#105#pop | simplis_pop1_105.sxgph
new#pop | simplis_pop1_100.sxgph