baseschematic: ..\..\..\..\..\5_multi_tone.sxsch
log_file: ..\..\..\dvm_advanced.log
simulator: simplis
screenshot: schematic.png
deck: input.deck
init: input.deck.init
test_argument: FindACSteadyState|DC Input|POP-AC
datetimestamp: 11/17/2016 11:13 AM
status: RUN
feature: DVM LOAD#tran
spec: Max_VLOAD=pass,Max. Output1 Voltage (400.171) is less than or equal to Max. Output1 Voltage Spec (420)
scalar: Frequency(SRC)=50
scalar: RMS(VSRC)=114.274
scalar: VLOAD %_diff_last_2_linecycles=0.000000753023%
spec: AC_Settling(LOAD)=pass, Voltage across LOAD has settled to (7.53023n) % and is less than or equal to Max Settling Spec of (10m) %
scalar: Avg(VLOAD Last LineCycle)=400.082
scalar: Avg(VLOAD Previous LineCycle)=400.082
scalar: VLOAD %_diff_last_2_linecycles=0.000000753023%
scalar: Avg(VLOAD At Simulation Start Time)=400.082
stats: N/A
numgraphs: 6
graphid: 1
graphname: AC#tran
sg: simplis_tran1_1
path: simplis_tran1_1.sxgph
graphid: 6
graphname: SIGNAL#tran
sg: simplis_tran1_6
path: simplis_tran1_6.sxgph
graphid: 11
graphname: default#11#tran
sg: simplis_tran1_11
path: simplis_tran1_11.sxgph
graphid: 20
graphname: RAMP#tran
sg: simplis_tran1_20
path: simplis_tran1_20.sxgph
scalar: Max(VSRC)=114.275
scalar: Min(VSRC)=114.274
scalar: Min(ISRC)=1.81368
scalar: Max(ISRC)=1.81468
graphid: 27
graphname: DVM SRC#tran
sg: simplis_tran1_27
path: simplis_tran1_27.sxgph
curve31:VSRC,FF0000
curve37:ISRC,008000
png: simplis_tran1_27.png
scalar: Max(VLOAD)=400.171
scalar: Min(VLOAD)=400.063
scalar: Max(ILOAD)=500.214m
scalar: Min(ILOAD)=500.079m
graphid: 32
graphname: DVM LOAD#tran
sg: simplis_tran1_32
path: simplis_tran1_32.sxgph
curve36:VLOAD,FF0000
curve39:ILOAD,008000
png: simplis_tran1_32.png
rstatus: PASS
