baseschematic: ..\..\..\..\..\5_multi_tone.sxsch
log_file: ..\..\..\dvm_advanced.log
simulator: simplis
screenshot: schematic.png
deck: input.deck
init: input.deck.init
test_argument: Bode Plot|DC Input|POP-AC
datetimestamp: 11/17/2016 11:16 AM
status: RUN
scalar: Power(SRC)=207.314
scalar: Power(LOAD)=200.089
scalar: Efficiency=96.5149%
feature: DVM Bode Plot#log#ac,100
spec: Min_VLOAD=pass,Min. Output1 Voltage (400.063) is greater than or equal to Min. Output1 Voltage Spec (380)
spec: Max_VLOAD=pass,Max. Output1 Voltage (400.171) is less than or equal to Max. Output1 Voltage Spec (420)
stats: N/A
numgraphs: 10
scalar: min_phase=23.3146
scalar: min_phase_freq=50
scalar: phase_crossover_freq=Unable to determine phase_crossover_freq
scalar: phase_margin=65.7001
scalar: gain_crossover_freq=9.19732
scalar: gain_margin=Unable to determine gain_margin
graphid: 101
graphname: DVM Bode Plot#log#ac
sg: simplis_ac1_101
path: simplis_ac1_101.sxgph
curve105:PHASE,FF0000
curve106:GAIN,008000
png: simplis_ac1_101.png
graphid: 41
graphname: AC#pop
sg: simplis_pop1_41
path: simplis_pop1_41.sxgph
graphid: 46
graphname: SIGNAL#pop
sg: simplis_pop1_46
path: simplis_pop1_46.sxgph
graphid: 51
graphname: default#51#pop
sg: simplis_pop1_51
path: simplis_pop1_51.sxgph
graphid: 60
graphname: RAMP#pop
sg: simplis_pop1_60
path: simplis_pop1_60.sxgph
scalar: Max(VSRC)=114.275
scalar: Avg(VSRC)=114.274
scalar: Min(VSRC)=114.274
scalar: Pk2Pk(VSRC)=401.519u
scalar: RMS(VSRC)=114.274
scalar: RMS(ISRC)=1.81418
scalar: Pk2Pk(ISRC)=1.0038m
scalar: Min(ISRC)=1.81368
scalar: Avg(ISRC)=1.81418
scalar: Max(ISRC)=1.81468
graphid: 67
graphname: DVM SRC#pop
sg: simplis_pop1_67
path: simplis_pop1_67.sxgph
curve71:VSRC,FF0000
curve77:ISRC,008000
png: simplis_pop1_67.png
scalar: Max(VLOAD)=400.171
scalar: Avg(VLOAD)=400.089
scalar: Min(VLOAD)=400.063
scalar: Pk2Pk(VLOAD)=107.592m
scalar: RMS(VLOAD)=400.089
scalar: Max(ILOAD)=500.213m
scalar: Avg(ILOAD)=500.111m
scalar: Min(ILOAD)=500.079m
scalar: Pk2Pk(ILOAD)=134.49u
scalar: RMS(ILOAD)=500.111m
graphid: 72
graphname: DVM LOAD#pop
sg: simplis_pop1_72
path: simplis_pop1_72.sxgph
curve76:VLOAD,FF0000
curve79:ILOAD,008000
png: simplis_pop1_72.png
graphid: 81
graphname: SIGNAL#log#ac
sg: simplis_ac1_81
path: simplis_ac1_81.sxgph
graphid: 88
graphname: AC#log#ac
sg: simplis_ac1_88
path: simplis_ac1_88.sxgph
graphid: 94
graphname: RAMP#log#ac
sg: simplis_ac1_94
path: simplis_ac1_94.sxgph
spec: min_gain_margin=warn,Unable to determine min_gain_margin
spec: min_phase_margin=pass,Phase Margin (65.7001) is greater than Min. Phase Margin (35)
rstatus: WARN
