baseschematic: ..\..\..\..\..\..\4_multi_tone.sxsch
log_file: ..\..\..\..\dvm_advanced.log
simulator: simplis
screenshot: schematic.png
deck: input.deck
init: input.deck.init
test_argument: Bode Plot|AC Input|Multi-Tone|NLB multiplier
datetimestamp: 11/17/2016 11:31 AM
status: RUN
spec: Min_VLOAD=pass,Min. Output1 Voltage (393.905) is greater than or equal to Min. Output1 Voltage Spec (380)
spec: Max_VLOAD=pass,Max. Output1 Voltage (405.685) is less than or equal to Max. Output1 Voltage Spec (420)
stats: N/A
numgraphs: 6
graphid: 138
graphname: new#tran
sg: simplis_tran4_138
path: simplis_tran4_138.sxgph
graphid: 143
graphname: default#143#tran
sg: simplis_tran4_143
path: simplis_tran4_143.sxgph
scalar: Max(VSRC)=161.628
scalar: Avg(VSRC)=-1.55903m
scalar: Min(VSRC)=-161.618
scalar: Pk2Pk(VSRC)=323.245
scalar: RMS(VSRC)=114.26
scalar: RMS(ISRC)=1.83539
scalar: Pk2Pk(ISRC)=5.42928
scalar: Min(ISRC)=-2.69503
scalar: Avg(ISRC)=3.8981m
scalar: Max(ISRC)=2.73426
graphid: 148
graphname: DVM SRC#tran
sg: simplis_tran4_148
path: simplis_tran4_148.sxgph
curve152:VSRC,FF0000
curve158:ISRC,008000
png: simplis_tran4_148.png
scalar: Max(VLOAD)=405.685
scalar: Avg(VLOAD)=400.093
scalar: Min(VLOAD)=393.905
scalar: Pk2Pk(VLOAD)=11.7802
scalar: RMS(VLOAD)=400.106
scalar: Max(ILOAD)=507.106m
scalar: Avg(ILOAD)=500.116m
scalar: Min(ILOAD)=492.381m
scalar: Pk2Pk(ILOAD)=14.7252m
scalar: RMS(ILOAD)=500.133m
graphid: 153
graphname: DVM LOAD#tran
sg: simplis_tran4_153
path: simplis_tran4_153.sxgph
curve157:VLOAD,FF0000
curve160:ILOAD,008000
png: simplis_tran4_153.png
graphid: 162
graphname: AC#tran
sg: simplis_tran4_162
path: simplis_tran4_162.sxgph
curve166:IL,FF0000
png: simplis_tran4_162.png
scalar: min_phase=12.6058
scalar: min_phase_freq=45
scalar: phase_crossover_freq=Unable to determine phase_crossover_freq
scalar: phase_margin=47.9822
scalar: gain_crossover_freq=11.3713
scalar: gain_margin=Unable to determine gain_margin
graphid: 168
graphname: DVM Bode Plot
sg: simplis_Multi_ToneAC2_168
path: simplis_Multi_ToneAC2_168.sxgph
curve172:PHASE,FF0000
curve174:GAIN,008000
png: simplis_Multi_ToneAC2_168.png
spec: min_gain_margin=warn,Unable to determine min_gain_margin
spec: min_phase_margin=pass,Phase Margin (47.9822) is greater than Min. Phase Margin (35)
rstatus: WARN
