baseschematic: ..\..\..\..\..\..\4_multi_tone.sxsch
log_file: ..\..\..\..\dvm_advanced.log
simulator: simplis
screenshot: schematic.png
deck: input.deck
init: input.deck.init
test_argument: Bode Plot|DC Input|POP-AC|PWM multiplier
datetimestamp: 11/17/2016 11:30 AM
status: RUN
scalar: Power(SRC)=210.415
scalar: Power(LOAD)=200.093
scalar: Efficiency=95.0946%
feature: DVM Bode Plot#log#ac,100
spec: Min_VLOAD=pass,Min. Output1 Voltage (400.068) is greater than or equal to Min. Output1 Voltage Spec (380)
spec: Max_VLOAD=pass,Max. Output1 Voltage (400.138) is less than or equal to Max. Output1 Voltage Spec (420)
stats: N/A
numgraphs: 6
graphid: 105
graphname: default#105#pop
sg: simplis_pop1_105
path: simplis_pop1_105.sxgph
scalar: Max(VSRC)=114.263
scalar: Avg(VSRC)=114.263
scalar: Min(VSRC)=114.263
scalar: Pk2Pk(VSRC)=40.5387u
scalar: RMS(VSRC)=114.263
scalar: RMS(ISRC)=1.84149
scalar: Pk2Pk(ISRC)=101.347u
scalar: Min(ISRC)=1.84144
scalar: Avg(ISRC)=1.84149
scalar: Max(ISRC)=1.84154
graphid: 111
graphname: DVM SRC#pop
sg: simplis_pop1_111
path: simplis_pop1_111.sxgph
curve115:VSRC,FF0000
curve121:ISRC,008000
png: simplis_pop1_111.png
scalar: Max(VLOAD)=400.138
scalar: Avg(VLOAD)=400.093
scalar: Min(VLOAD)=400.068
scalar: Pk2Pk(VLOAD)=70.1029m
scalar: RMS(VLOAD)=400.093
scalar: Max(ILOAD)=500.172m
scalar: Avg(ILOAD)=500.116m
scalar: Min(ILOAD)=500.085m
scalar: Pk2Pk(ILOAD)=87.6286u
scalar: RMS(ILOAD)=500.116m
graphid: 116
graphname: DVM LOAD#pop
sg: simplis_pop1_116
path: simplis_pop1_116.sxgph
curve120:VLOAD,FF0000
curve123:ILOAD,008000
png: simplis_pop1_116.png
graphid: 125
graphname: AC#pop
sg: simplis_pop1_125
path: simplis_pop1_125.sxgph
curve129:IL,FF0000
png: simplis_pop1_125.png
scalar: min_phase=10.7993
scalar: min_phase_freq=50
scalar: phase_crossover_freq=Unable to determine phase_crossover_freq
scalar: phase_margin=49.131
scalar: gain_crossover_freq=11.3576
scalar: gain_margin=Unable to determine gain_margin
graphid: 131
graphname: DVM Bode Plot#log#ac
sg: simplis_ac1_131
path: simplis_ac1_131.sxgph
curve135:PHASE,FF0000
curve136:GAIN,008000
png: simplis_ac1_131.png
graphid: 100
graphname: new#pop
sg: simplis_pop1_100
path: simplis_pop1_100.sxgph
spec: min_gain_margin=warn,Unable to determine min_gain_margin
spec: min_phase_margin=pass,Phase Margin (49.131) is greater than Min. Phase Margin (35)
rstatus: WARN
