baseschematic: ..\..\..\..\..\5_multi_tone.sxsch
log_file: ..\..\..\dvm_advanced.log
simulator: simplis
screenshot: schematic.png
deck: input.deck
init: input.deck.init
test_argument: Bode Plot|AC Input|Multi-Tone
datetimestamp: 11/17/2016 11:17 AM
status: RUN
spec: Min_VLOAD=pass,Min. Output1 Voltage (394.23) is greater than or equal to Min. Output1 Voltage Spec (380)
spec: Max_VLOAD=pass,Max. Output1 Voltage (405.4) is less than or equal to Max. Output1 Voltage Spec (420)
stats: N/A
numgraphs: 7
graphid: 108
graphname: AC#tran
sg: simplis_tran2_108
path: simplis_tran2_108.sxgph
graphid: 113
graphname: SIGNAL#tran
sg: simplis_tran2_113
path: simplis_tran2_113.sxgph
graphid: 118
graphname: default#118#tran
sg: simplis_tran2_118
path: simplis_tran2_118.sxgph
graphid: 127
graphname: RAMP#tran
sg: simplis_tran2_127
path: simplis_tran2_127.sxgph
scalar: Max(VSRC)=161.621
scalar: Avg(VSRC)=-2.15802m
scalar: Min(VSRC)=-161.624
scalar: Pk2Pk(VSRC)=323.245
scalar: RMS(VSRC)=114.262
scalar: RMS(ISRC)=1.81208
scalar: Pk2Pk(ISRC)=5.35982
scalar: Min(ISRC)=-2.67534
scalar: Avg(ISRC)=5.46282m
scalar: Max(ISRC)=2.68448
graphid: 134
graphname: DVM SRC#tran
sg: simplis_tran2_134
path: simplis_tran2_134.sxgph
curve138:VSRC,FF0000
curve144:ISRC,008000
png: simplis_tran2_134.png
scalar: Max(VLOAD)=405.4
scalar: Avg(VLOAD)=400.081
scalar: Min(VLOAD)=394.23
scalar: Pk2Pk(VLOAD)=11.1698
scalar: RMS(VLOAD)=400.094
scalar: Max(ILOAD)=506.75m
scalar: Avg(ILOAD)=500.102m
scalar: Min(ILOAD)=492.787m
scalar: Pk2Pk(ILOAD)=13.9622m
scalar: RMS(ILOAD)=500.118m
graphid: 139
graphname: DVM LOAD#tran
sg: simplis_tran2_139
path: simplis_tran2_139.sxgph
curve143:VLOAD,FF0000
curve146:ILOAD,008000
png: simplis_tran2_139.png
scalar: min_phase=25.4149
scalar: min_phase_freq=45
scalar: phase_crossover_freq=Unable to determine phase_crossover_freq
scalar: phase_margin=65.0557
scalar: gain_crossover_freq=9.53423
scalar: gain_margin=Unable to determine gain_margin
graphid: 148
graphname: DVM Bode Plot
sg: simplis_Multi_ToneAC1_148
path: simplis_Multi_ToneAC1_148.sxgph
curve152:PHASE,FF0000
curve154:GAIN,008000
png: simplis_Multi_ToneAC1_148.png
spec: min_gain_margin=warn,Unable to determine min_gain_margin
spec: min_phase_margin=pass,Phase Margin (65.0557) is greater than Min. Phase Margin (35)
rstatus: WARN
