back to overview ▲

### » DVM Test Report: FindACSteadyState|AC Input|POP_AC|PWM multiplier

Test Details |
Schematic | 4_multi_tone.sxsch
Test | FindACSteadyState|AC Input|POP_AC|PWM multiplier
Date / Time | 11/17/2016 11:29 AM
Report Directory | DVM_REPORTS\2016-11-17-11_20_AM\FindACSteadyState\AC Input\POP_AC\PWM multiplier
Log File | report.txt
Screenshot | schematic.png
Status | PASS
Simulator | simplis
Deck | input.deck
Init | input.deck.init
Measured Scalar Values |
Frequency(SRC) | 50
ILOAD | MIN 494.426m MAX 505.812m
ISRC | MIN -2.63229 MAX 2.63229
VLOAD | MIN 395.541 MAX 404.65
VLOAD %_diff_last_2_linecycles | 0.00000000106541%
VLOAD At Simulation Start Time | AVG 400.093
VLOAD Last LineCycle | AVG 400.093
VLOAD Previous LineCycle | AVG 400.093
VSRC | MIN -161.579 MAX 161.579 RMS 115
Measured Spec Values |
AC_Settling(LOAD) | PASS: Voltage across LOAD has settled to (10.6541p) % and is less than or equal to Max Settling Spec of (10m) %
Max_VLOAD | PASS: Max. Output1 Voltage (404.65) is less than or equal to Max. Output1 Voltage Spec (420)
LOAD VLOAD ILOAD
SXGPH File | simplis_tran2_48.sxgph
AC IL
SXGPH File | simplis_tran2_57.sxgph
SRC VSRC ISRC
SXGPH File | simplis_tran2_43.sxgph
Other SXGPH Files |
new#tran | simplis_tran2_32.sxgph
default#37#tran | simplis_tran2_37.sxgph