### » SIMPLIS DVM Test Report Overview

General |
Schematic | 5_multi_tone.sxsch
Testplan | dvm_advanced.testplan
Original Testplan Filename | 5_multi_tone.testplan
Date / Time | 2016-11-17 11:12 AM
Report Directory | DVM_REPORTS\2016-11-17-11_12_AM
Log File | dvm_advanced.log
# of Tests Run | 5 of 5 (5 of 5 Run, 1 Passed, 0 Failed, 2 Ran with Warnings, 1 Skipped)
Total Time | 5m 12s
Design Specifications |
Circuit Name | 5_multi_tone
Description | Critical Conducton Mode Multi-Tone
Input 1 (Low Line) | 115 VRMS Nominal (85 VRMS to 132 VRMS)
Input 1 (High Line) | 230 VRMS Nominal (170 VRMS to 265 VRMS)
Output 1 | 400 V (±5%) @ 500m A
Low Frequency | 50Hz
High Frequency | 60Hz
Switching Frequency | 100KHz
Excel-compatible Results |
Scalar Results | dvm_advanced_table_scalars.txt
Spec Results | dvm_advanced_table_specs.txt
Statistic Results | dvm_advanced_table_statistics.txt
Statistic Specs | dvm_advanced_table_statspecs.txt
Overview Graphs |
Pop-AC to Multi-Tone Comparison Multi Tone AC Input Multi Tone AC Input POP/AC DC Input POP/AC DC Input
SXGPH File | global_163.sxgph
Source Test | Bode Plot|Generate Summary Curves
Test 1 of 5 | top ▲
Test Label | FindACSteadyState|DC Input|POP-AC
Simulator | simplis
Test Report | FindACSteadyState\DC Input\POP-AC\report.txt.html
Status | PASS
Test Time | 1m 39s
Test 2 of 5 | top ▲
Test Label | FindACSteadyState|AC Input|Multi-Tone
Simulator | simplis
Test Report | FindACSteadyState\AC Input\Multi-Tone\report.txt.html
Status | RUN
Test Time | 2m 35s
Test 3 of 5 | top ▲
Test Label | Bode Plot|DC Input|POP-AC
Simulator | simplis
Test Report | Bode Plot\DC Input\POP-AC\report.txt.html
Status | WARN
Test Time | 8s
Test 4 of 5 | top ▲
Test Label | Bode Plot|AC Input|Multi-Tone
Simulator | simplis
Test Report | Bode Plot\AC Input\Multi-Tone\report.txt.html
Status | WARN
Test Time | 46s
Test 5 of 5 | top ▲
Test Label | Bode Plot|Generate Summary Curves
Simulator | N/A
Test Report | Bode Plot\Generate Summary Curves\report.txt.html
Status | SKIP
Test Time | 2s