back to overview ▲

### » DVM Test Report: Bode Plot|DC Input|Multi-Tone|NLB multiplier

Test Details |
Schematic | 4_multi_tone.sxsch
Test | Bode Plot|DC Input|Multi-Tone|NLB multiplier
Date / Time | 11/17/2016 11:29 AM
Report Directory | DVM_REPORTS\2016-11-17-11_20_AM\Bode Plot\DC Input\Multi-Tone\NLB multiplier
Log File | report.txt
Screenshot | schematic.png
Status | WARN
Simulator | simplis
Deck | input.deck
Init | input.deck.init
Measured Scalar Values |
gain_crossover_freq | 11.2477
gain_margin | Unable to determine gain_margin
ILOAD | AVG 500.116m MIN 498.074m MAX 501.43m RMS 500.117m PK2PK 3.35616m
ISRC | AVG 1.84153 MIN 1.7646 MAX 1.91219 RMS 1.84198 PK2PK 147.59m
min_phase | 10.9935
min_phase_freq | 50
phase_crossover_freq | Unable to determine phase_crossover_freq
phase_margin | 48.3828
VLOAD | AVG 400.093 MIN 398.459 MAX 401.144 RMS 400.094 PK2PK 2.68493
VSRC | AVG 114.263 MIN 114.235 MAX 114.294 RMS 114.263 PK2PK 59.0359m
Measured Spec Values |
Max_VLOAD | PASS: Max. Output1 Voltage (401.144) is less than or equal to Max. Output1 Voltage Spec (420)
Min_VLOAD | PASS: Min. Output1 Voltage (398.459) is greater than or equal to Min. Output1 Voltage Spec (380)
min_gain_margin | WARN: Unable to determine min_gain_margin
min_phase_margin | PASS: Phase Margin (48.3828) is greater than Min. Phase Margin (35)
AC IL
SXGPH File | simplis_tran3_87.sxgph
Bode Plot GAIN PHASE
SXGPH File | simplis_Multi_ToneAC1_93.sxgph
LOAD VLOAD ILOAD
SXGPH File | simplis_tran3_78.sxgph
SRC VSRC ISRC
SXGPH File | simplis_tran3_73.sxgph
Other SXGPH Files |
new#tran | simplis_tran3_63.sxgph
default#68#tran | simplis_tran3_68.sxgph