back to overview ▲

### » DVM Test Report: Bode Plot|AC Input|Multi-Tone

Test Details |
Schematic | 5_multi_tone.sxsch
Test | Bode Plot|AC Input|Multi-Tone
Date / Time | 11/17/2016 11:17 AM
Report Directory | DVM_REPORTS\2016-11-17-11_12_AM\Bode Plot\AC Input\Multi-Tone
Log File | report.txt
Screenshot | schematic.png
Status | WARN
Simulator | simplis
Deck | input.deck
Init | input.deck.init
Measured Scalar Values |
gain_crossover_freq | 9.53423
gain_margin | Unable to determine gain_margin
ILOAD | AVG 500.102m MIN 492.787m MAX 506.75m RMS 500.118m PK2PK 13.9622m
ISRC | AVG 5.46282m MIN -2.67534 MAX 2.68448 RMS 1.81208 PK2PK 5.35982
min_phase | 25.4149
min_phase_freq | 45
phase_crossover_freq | Unable to determine phase_crossover_freq
phase_margin | 65.0557
VLOAD | AVG 400.081 MIN 394.23 MAX 405.4 RMS 400.094 PK2PK 11.1698
VSRC | AVG -2.15802m MIN -161.624 MAX 161.621 RMS 114.262 PK2PK 323.245
Measured Spec Values |
Max_VLOAD | PASS: Max. Output1 Voltage (405.4) is less than or equal to Max. Output1 Voltage Spec (420)
Min_VLOAD | PASS: Min. Output1 Voltage (394.23) is greater than or equal to Min. Output1 Voltage Spec (380)
min_gain_margin | WARN: Unable to determine min_gain_margin
min_phase_margin | PASS: Phase Margin (65.0557) is greater than Min. Phase Margin (35)
Bode Plot GAIN PHASE
SXGPH File | simplis_Multi_ToneAC1_148.sxgph
LOAD VLOAD ILOAD
SXGPH File | simplis_tran2_139.sxgph
SRC VSRC ISRC
SXGPH File | simplis_tran2_134.sxgph
Other SXGPH Files |
AC#tran | simplis_tran2_108.sxgph
SIGNAL#tran | simplis_tran2_113.sxgph
default#118#tran | simplis_tran2_118.sxgph
RAMP#tran | simplis_tran2_127.sxgph