baseschematic: ..\..\..\..\..\..\4_multi_tone.sxsch
log_file: ..\..\..\..\dvm_advanced.log
simulator: simplis
screenshot: schematic.png
deck: input.deck
init: input.deck.init
test_argument: Bode Plot|AC Input|POP-AC|PWM multiplier
datetimestamp: 11/17/2016 11:32 AM
status: RUN
scalar: Power(SRC)=209.61
scalar: Power(LOAD)=200.106
scalar: Efficiency=95.4659%
feature: DVM Bode Plot#log#ac,100
spec: Min_VLOAD=pass,Min. Output1 Voltage (395.541) is greater than or equal to Min. Output1 Voltage Spec (380)
spec: Max_VLOAD=pass,Max. Output1 Voltage (404.65) is less than or equal to Max. Output1 Voltage Spec (420)
stats: N/A
numgraphs: 6
scalar: min_phase=9.82901
scalar: min_phase_freq=50
scalar: phase_crossover_freq=Unable to determine phase_crossover_freq
scalar: phase_margin=48.8065
scalar: gain_crossover_freq=11.4795
scalar: gain_margin=Unable to determine gain_margin
graphid: 206
graphname: DVM Bode Plot#log#ac
sg: simplis_ac2_206
path: simplis_ac2_206.sxgph
curve210:PHASE,FF0000
curve211:GAIN,008000
png: simplis_ac2_206.png
graphid: 175
graphname: new#pop
sg: simplis_pop2_175
path: simplis_pop2_175.sxgph
graphid: 180
graphname: default#180#pop
sg: simplis_pop2_180
path: simplis_pop2_180.sxgph
scalar: Max(VSRC)=161.579
scalar: Avg(VSRC)=-44.9339n
scalar: Min(VSRC)=-161.579
scalar: Pk2Pk(VSRC)=323.158
scalar: RMS(VSRC)=114.257
scalar: RMS(ISRC)=1.83507
scalar: Pk2Pk(ISRC)=5.26458
scalar: Min(ISRC)=-2.63229
scalar: Avg(ISRC)=8.3149n
scalar: Max(ISRC)=2.63229
graphid: 186
graphname: DVM SRC#pop
sg: simplis_pop2_186
path: simplis_pop2_186.sxgph
curve190:VSRC,FF0000
curve196:ISRC,008000
png: simplis_pop2_186.png
scalar: Max(VLOAD)=404.65
scalar: Avg(VLOAD)=400.093
scalar: Min(VLOAD)=395.541
scalar: Pk2Pk(VLOAD)=9.10904
scalar: RMS(VLOAD)=400.106
scalar: Max(ILOAD)=505.812m
scalar: Avg(ILOAD)=500.116m
scalar: Min(ILOAD)=494.426m
scalar: Pk2Pk(ILOAD)=11.3863m
scalar: RMS(ILOAD)=500.132m
graphid: 191
graphname: DVM LOAD#pop
sg: simplis_pop2_191
path: simplis_pop2_191.sxgph
curve195:VLOAD,FF0000
curve198:ILOAD,008000
png: simplis_pop2_191.png
graphid: 200
graphname: AC#pop
sg: simplis_pop2_200
path: simplis_pop2_200.sxgph
curve204:IL,FF0000
png: simplis_pop2_200.png
spec: min_gain_margin=warn,Unable to determine min_gain_margin
spec: min_phase_margin=pass,Phase Margin (48.8065) is greater than Min. Phase Margin (35)
rstatus: WARN
