back to overview ▲

### » DVM Test Report: Bode Plot|DC Input|POP-AC

Test Details |
Schematic | 5_multi_tone.sxsch
Test | Bode Plot|DC Input|POP-AC
Date / Time | 11/17/2016 11:16 AM
Report Directory | DVM_REPORTS\2016-11-17-11_12_AM\Bode Plot\DC Input\POP-AC
Log File | report.txt
Screenshot | schematic.png
Status | WARN
Simulator | simplis
Deck | input.deck
Init | input.deck.init
Measured Scalar Values |
Efficiency | 96.5149%
gain_crossover_freq | 9.19732
gain_margin | Unable to determine gain_margin
ILOAD | AVG 500.111m MIN 500.079m MAX 500.213m RMS 500.111m PK2PK 134.49u
ISRC | AVG 1.81418 MIN 1.81368 MAX 1.81468 RMS 1.81418 PK2PK 1.0038m
min_phase | 23.3146
min_phase_freq | 50
phase_crossover_freq | Unable to determine phase_crossover_freq
phase_margin | 65.7001
Power(LOAD) | 200.089
Power(SRC) | 207.314
VLOAD | AVG 400.089 MIN 400.063 MAX 400.171 RMS 400.089 PK2PK 107.592m
VSRC | AVG 114.274 MIN 114.274 MAX 114.275 RMS 114.274 PK2PK 401.519u
Measured Spec Values |
Max_VLOAD | PASS: Max. Output1 Voltage (400.171) is less than or equal to Max. Output1 Voltage Spec (420)
Min_VLOAD | PASS: Min. Output1 Voltage (400.063) is greater than or equal to Min. Output1 Voltage Spec (380)
min_gain_margin | WARN: Unable to determine min_gain_margin
min_phase_margin | PASS: Phase Margin (65.7001) is greater than Min. Phase Margin (35)
Bode Plot GAIN PHASE
SXGPH File | simplis_ac1_101.sxgph
LOAD VLOAD ILOAD
SXGPH File | simplis_pop1_72.sxgph
SRC VSRC ISRC
SXGPH File | simplis_pop1_67.sxgph
Other SXGPH Files |
AC#pop | simplis_pop1_41.sxgph
SIGNAL#pop | simplis_pop1_46.sxgph
default#51#pop | simplis_pop1_51.sxgph
RAMP#pop | simplis_pop1_60.sxgph
SIGNAL#log#ac | simplis_ac1_81.sxgph
AC#log#ac | simplis_ac1_88.sxgph
RAMP#log#ac | simplis_ac1_94.sxgph