back to overview ▲

### » DVM Test Report: Bode Plot|AC Input|POP-AC|PWM multiplier

Test Details |
Schematic | 4_multi_tone.sxsch
Test | Bode Plot|AC Input|POP-AC|PWM multiplier
Date / Time | 11/17/2016 11:32 AM
Report Directory | DVM_REPORTS\2016-11-17-11_20_AM\Bode Plot\AC Input\POP-AC\PWM multiplier
Log File | report.txt
Screenshot | schematic.png
Status | WARN
Simulator | simplis
Deck | input.deck
Init | input.deck.init
Measured Scalar Values |
Efficiency | 95.4659%
gain_crossover_freq | 11.4795
gain_margin | Unable to determine gain_margin
ILOAD | AVG 500.116m MIN 494.426m MAX 505.812m RMS 500.132m PK2PK 11.3863m
ISRC | AVG 8.3149n MIN -2.63229 MAX 2.63229 RMS 1.83507 PK2PK 5.26458
min_phase | 9.82901
min_phase_freq | 50
phase_crossover_freq | Unable to determine phase_crossover_freq
phase_margin | 48.8065
Power(LOAD) | 200.106
Power(SRC) | 209.61
VLOAD | AVG 400.093 MIN 395.541 MAX 404.65 RMS 400.106 PK2PK 9.10904
VSRC | AVG -44.9339n MIN -161.579 MAX 161.579 RMS 114.257 PK2PK 323.158
Measured Spec Values |
Max_VLOAD | PASS: Max. Output1 Voltage (404.65) is less than or equal to Max. Output1 Voltage Spec (420)
Min_VLOAD | PASS: Min. Output1 Voltage (395.541) is greater than or equal to Min. Output1 Voltage Spec (380)
min_gain_margin | WARN: Unable to determine min_gain_margin
min_phase_margin | PASS: Phase Margin (48.8065) is greater than Min. Phase Margin (35)
Bode Plot GAIN PHASE
SXGPH File | simplis_ac2_206.sxgph
AC IL
SXGPH File | simplis_pop2_200.sxgph
LOAD VLOAD ILOAD
SXGPH File | simplis_pop2_191.sxgph
SRC VSRC ISRC
SXGPH File | simplis_pop2_186.sxgph
Other SXGPH Files |
new#pop | simplis_pop2_175.sxgph
default#180#pop | simplis_pop2_180.sxgph