back to overview ▲

### » DVM Test Report: Bode Plot|AC Input|Multi-Tone|NLB multiplier

Test Details |
Schematic | 4_multi_tone.sxsch
Test | Bode Plot|AC Input|Multi-Tone|NLB multiplier
Date / Time | 11/17/2016 11:31 AM
Report Directory | DVM_REPORTS\2016-11-17-11_20_AM\Bode Plot\AC Input\Multi-Tone\NLB multiplier
Log File | report.txt
Screenshot | schematic.png
Status | WARN
Simulator | simplis
Deck | input.deck
Init | input.deck.init
Measured Scalar Values |
gain_crossover_freq | 11.3713
gain_margin | Unable to determine gain_margin
ILOAD | AVG 500.116m MIN 492.381m MAX 507.106m RMS 500.133m PK2PK 14.7252m
ISRC | AVG 3.8981m MIN -2.69503 MAX 2.73426 RMS 1.83539 PK2PK 5.42928
min_phase | 12.6058
min_phase_freq | 45
phase_crossover_freq | Unable to determine phase_crossover_freq
phase_margin | 47.9822
VLOAD | AVG 400.093 MIN 393.905 MAX 405.685 RMS 400.106 PK2PK 11.7802
VSRC | AVG -1.55903m MIN -161.618 MAX 161.628 RMS 114.26 PK2PK 323.245
Measured Spec Values |
Max_VLOAD | PASS: Max. Output1 Voltage (405.685) is less than or equal to Max. Output1 Voltage Spec (420)
Min_VLOAD | PASS: Min. Output1 Voltage (393.905) is greater than or equal to Min. Output1 Voltage Spec (380)
min_gain_margin | WARN: Unable to determine min_gain_margin
min_phase_margin | PASS: Phase Margin (47.9822) is greater than Min. Phase Margin (35)
AC IL
SXGPH File | simplis_tran4_162.sxgph
Bode Plot GAIN PHASE
SXGPH File | simplis_Multi_ToneAC2_168.sxgph
LOAD VLOAD ILOAD
SXGPH File | simplis_tran4_153.sxgph
SRC VSRC ISRC
SXGPH File | simplis_tran4_148.sxgph
Other SXGPH Files |
new#tran | simplis_tran4_138.sxgph
default#143#tran | simplis_tran4_143.sxgph