For this simple example, the auto-generation features will be used to create a digital VCO. The end device should meet the following spec:

inputs: Base Frequency (32-bit Unsigned Integer) Exponent (4-bit Unsigned Integer) Ready output: OUT | parameters: IC DELAY (Double) DUTY_CYCLE (Double)
The digital VCO should create a digital output signal whose frequency is such that: `FREQ = BASE * (10 ^ EXPONENT)` (open .sxsch)